| OrbbecSDK 1.5.7 OrbbecSDK: Software-Development-Kit for Orbbec 3D-Sensor devices

- Main Page
- Namespaces
- Classes
- Files

- Class List
- Class Index
- Class Hierarchy
- Class Members

Public Attributes | List of all members
OBDeviceIpAddrConfig Struct Reference

网络设备的 IP 地址配置（ipv4） More...

`#include <ObTypes.h>`

## Public Attributes
uint16_t | dhcp
| dhcp 动态 ip 配置开关; 0: 关; 1: 开 More...
uint8_t | address [4]
| ip 地址 (大端模式, 如 192.168.1.1，则 address[0]==192) More...
uint8_t | mask [4]
| 子网掩码 (大端模式) More...
uint8_t | gateway [4]
| 网关 (大端模式) More...

## Detailed Description

网络设备的 IP 地址配置（ipv4）

Definition at line 1157 of file ObTypes.h.

## Member Data Documentation

uint16_t OBDeviceIpAddrConfig::dhcp

dhcp 动态 ip 配置开关; 0: 关; 1: 开

Definition at line 1158 of file ObTypes.h.

uint8_t OBDeviceIpAddrConfig::address[4]

ip 地址 (大端模式, 如 192.168.1.1，则 address[0]==192)

Definition at line 1159 of file ObTypes.h.

uint8_t OBDeviceIpAddrConfig::mask[4]

子网掩码 (大端模式)

Definition at line 1160 of file ObTypes.h.

uint8_t OBDeviceIpAddrConfig::gateway[4]

网关 (大端模式)

Definition at line 1161 of file ObTypes.h.

The documentation for this struct was generated from the following file:

- /root/libobsensor/include/libobsensor/h/ObTypes.h